NOTES TO INSTALL NORTHERN TRUST DIAL UP MODEM CONNECTION

AT WORKSTATIONS USING SAPS SERVER

First Step

Place SAPS for Win 95 diskette in drive A of the workstation

Run install.exe

Select pool, add, add

\\BRADLEY\COM3 then select add again using \\BRADLEY\COM4

Set to disco after 10 min

No to read file

Continue with Next's till finished

Second Step

Through My Computer, add Northern Script directory to C drive

Remove diskette, insert Northern Trust CD-ROM dated 10/1/99

(or copy from my drive C to network, temporarily)

Select Tools, Dial95

Copy Northern.scp to newly created Northern Script drive on C

Third Step

Using DOS prompt, at c:\windows type "edit hosts"

Add as the third line:

192.77.161.2 (tab) passport.at.tnt

Save and exit

Fourth Step

Double click on dial-up networking in My Computer

Follow the Wizard, using auto-find

Enter our area code 414 appropriately, nothing at second line

Continue entering Next's

Name it Norther Trust Dial Up

Enter their number at appropriate line:

312-630-1781

Continue entering Next's until finished

Fifth Step

Restart computer

Sixth Step

Double click on My Computer

Select Dial-up Northern Trust and right click for properties Select Scripting tab

Enter, by browsing, to select the file we copied there earlier (northern.scp)

Right click on icon and move it to desk top

Rename NTC Dial Up

Exit

Seventh Step, To Use

Double click on the NTC Dial Up icon

Open Passport accordingly.

When done, double click on the double monitor icon at bottom right of tool bar, next to the time; select disconnect.